MAC_PREFIX              = 00:10:19
POWER_DISSIPATED        = 10:0:1:100
POWER_CONSUMED          = 10:0:2:100
SUBSYSTEM_VENDOR_ID     = 14e4
SUBSYSTEM_DEVICE_ID     = 1644
PXE                     = disable
PXE_SPEED               = AUTO
WOL                     = disable
PRODUCT_NAME            = Broadcom Gigabit Ethernet Controller
PART_NUMBER             = BCM95700A7 
ENGINEERING_CHANGE      = 107070-26
MANUFACTURING_ID        = 1455
ASSET_TAG               = XYZ11334455
VOLTAGE_SOURCE          = 1.8
FORCE_PCI               = enable
PART_REVISION           = 01
LED_MODE                = PHY_MODE2
PHY_TYPE                = Copper
PHY_ID                  = 12343210
MAX_PCI_RETRY           = AUTO
ASF                     = disable
DUAL_MAC_MODE           = normal
MBA_BOOT_PROTOCOL       = rpl
MBA_BOOTSTRAP_TYPE      = INT18
MBA_DELAY_TIME          = 10
EXPANSION_ROM_SIZE      = 128K
DESIGN_TYPE             = NIC
mac                     = 1
pxe                     = disable
