***************************************************************************
*                                                                         *
*                      Accton Technology Corporation                      *
*   Packet Driver Installation for EN1207D-TX PCI Fast Ethernet Adapter   *
*                                                                         *
*            Copyright (C) 1998 by Accton Technology Corporation.         *
*                         All rights reserved.                            *
*                                                                         *
***************************************************************************


   Introduction:
   -------------
   This document describes the procedure to set up the Packet driver for
   Accton's EN1207D-TX PCI Fast Ethernet Adapter.


   Sample Configuration Files:
   ---------------------------
      AUTOEXEC.BAT
      ACCPKT 0x60

   Notes:
   ------
     1.  Load the packet driver using the software interrupt and any
         optional switches if required.

         Usage: ACCPKT [options] <software_int_no> [media type]

         Example: ACCPKT -i 0x7e

         The only required parameter is the software interrupt.  A packet
         driver needs to have a software interrupt assigned to it for other
         programs to access it. The recommended interrupt is 0x7e. If you need
         any of the options listed below, place them before the software
         interrupt on the command line.

         -i - Force driver to report itself as 802.3 instead of Ethernet II.
         -d - Delayed initialization.  Used for diskless booting
         -n - NetWare conversion.  Converts 802.3 packets into 8137 packets
         -w - Windows hack, obsoleted by winpkt
         -p - Promiscuous mode disable
         -h - Help
         -u - Uninstall

      2. Media type can be used to force the card to work at a specific
         speed and duplex mode. If no media type if specified, the
         driver will read the hardware configuration from EEPROM on the
         card. The hardware configuration can be modified by running
         'set1207d' on the driver disk.

      3. Type command: C:\ACCPKT 0x60, the screen will display the 
         following message:

         System: [345]86 processor, PCI bus, Two 8259s
         Packet driver software interrupt is 0x60
         Interrupt number is 0x9
         I/O port is 0x6100
         My Ethernet address is 52:54:4C:29:29:AD

      4. Installing Multiple LAN Adapters:

         If there are multiple network cards on the main board. you can
         run ACCPKT 0x60 directly, then the screen will display:

         Packet driver for EN1207D-TX, PCI version 1.02
         Copyright 1998 (c), Accton Technology Corp.

         There are 2 network cards on your main board :
         Card 1. IRQ= 0x9  I/O= 0x6100  NodeID= 52:54:4C:29:29:AD
         Card 2. IRQ= 0xA  I/O= 0x6000  NodeID= 52:54:4C:29:29:64
         Please select a Card No.(1-2): 1

         System: [345]86 processor, PCI bus, Two 8259s
         Packet driver software interrupt is 0x60
         Interrupt number is 0x9
         I/O port is 0x6100
         My Ethernet address is 52:54:4C:29:29:AD

      5. Installing multiple drivers:

         If you want to install multiple cards each connection to a different
         network, you have to install the driver multiple times, each with a
         different packet interrupt number. Then modify the 'ioaddr' variable
         in 'config.tel' to specify the packet inetrrupt you will use.



